
  Ether16 LAN Card Setup
  for AT&T UNIX SVR4.2.2
  ----------------------------------------------------------------- 
  Contents:

  Before You Begin
  Setup
  Technical Support

  --------------------------------------------------------------------------
  BEFORE YOU BEGIN
  --------------------------------------------------------------------------
  If your computer does NOT have a plug-and-play motherboard, 
  the following notes apply to you:

  1.  Before attempting to install the Ether16 LAN Card's network
      software drivers, you MUST configure the card's internal
      settings with the SETUP program included on Ether16 disk 1
      under the UTILITY directory.  Use the program to set the
      card's interrupt (IRQ) and I/O settings.  For directions
      on using SETUP, see your Ether16 user guide.
  
  2.  Most network software packages like Windows 95, Windows NT,
      Novell NetWare, etc., include a "generic" network driver
      that will work with a wide range of network cards.  This
      generic driver is called a "Novell NE2000" compatible driver,
      and it is fully supported by the Ether16 card.  If your 
      network software package asks you to choose the name of
      the network card you're installing from a list of available
      adapters, and you find "NE2000" or "Novell NE2000" listed,
      you don't need to follow the directions below---simply choose
      to install the NE2000 driver and the Ether16 Card will be
      ready for use.  THE ETHER16 IS ONLY NE2000 COMPATIBLE
      WHEN THE CARD'S PLUG-AND-PLAY MODE IS TURNED OFF.  If 
      your PC has a plug-and-play motherboard, and you wish to 
      use the generic NE2000 driver, you must run the Ether16 
      SETUP program and turn the card's plug-and-play mode off.

  
  Setup
  -----------------------------------------------------------------------

     Login to UNIX as the "root" user

     Insert Ether16 disk 1 into Drive A: (or B:) and execute the
     following commands to copy the AT&T UNIX drivers 
     into the unix volume:

        (for Drive A:)
        #doscp a:/at\&tunix/setup setup
        #chmod +x setup
        #./setup a:/at\&tunix

        (for Drive B:)
        #doscp b:/at\&tunix/setup setup
        #chmod +x setup
        #./setup b:/at\&tunix

     Next, install the driver:

        #cd /usr/lib/tcprt/eth
        #./d22e

        The following message appears:

        Do you wish to install or delete the network driver(i/d/q)?

      Answer "i" to install the adapter.
      
      Depending on the number of adapters installed in your system, the
      following prompts appear:

      Note: The IP address and sub-net masks may have to be obtained from the
            network administrator.

        /* first adapter installation */
        Do you want to configure Board_0? (y/n/q)    y
        Enter number of media selection [3]:         3
        Please enter the IP host name for the device d22e_0
                   (default:xx ) XXXX
        Please Initialize the IP Address for host XXXX:   n.n.n.n
        Configure host XXXX with default Ethernet (TM) ifconfig option?   yes

        /* second adapter installation */
        Do you want to configure Board_1? (y/n/q)    y(n)
        Enter number of media selection [3]:         3
        Please enter the IP host name for the device d22e_1
                   (default:xx ) YYYY
        Please Initialize the IP Address for host YYYY:   n.n.n.n
        Configure host YYYY with default Ethernet (TM) ifconfig option?   yes

        /* third adapter installation*/
        Repeat the previous steps ....

      Do you wish to relink the kernel now? (y/n/q)   y
      
      Reboot the system for all modifications to be activiated
      # shutdown -y -g0


  
  HOW TO GET TECHNICAL SUPPORT
  ------------------------------------------------------------------------
  There are a variety of methods that you can use to get FREE technical help 
  or sales information about Linksys products.
  
   Support Hotline    (949) 261-1288
   Fax                (949) 261-8868
   BBS                (949) 261-2888 (8-N-1)
   E-mail             support@linksys.com
   World Wide Web     http://www.linksys.com



          

