; PRAID Policies File Syntax Specification
; Copyright (c) IBM Corporation, 2005

; This file is meant to show the syntax of a PRAID policies file.
; The following rules apply to this syntax:
;  -- { } indicates that one of the values separated by '|' should be chosen.
;  --  +  indicates that you may list one or more values separated by a comma.
;  -- ( ) indicates an optional value.
;
; See the User Guide for more information on this syntax.
; The following files provide some working examples of policies files:
; -- template.ini - A complex policies file example.
; -- RAID1-5.ini  - Configures RAID controllers using RAID-1 on first two drives and RAID-5 with remaining drives.
; -- RAID5HSP.ini - Configures RAID controllers using RAID-5 with a hot-spare drive.

; Comment line

; The policy name (Required)
[Policy.name]

; Specify when to use this policy (Required)
AppliesTo.1 = { m:mtype | s:serial | c:contn | t:ctype | d:drives }+ | ALL 
AppliesTo.2 = { m:mtype | s:serial | c:contn | t:ctype | d:drives }+ | ALL 
AppliesTo.3 = { m:mtype | s:serial | c:contn | t:ctype | d:drives }+ | ALL
…

; Controller parameters (Advanced users)
RebuildRate = { HIGH | MEDIUM | LOW }
ReadAhead   = { ADAPTIVE | ON | OFF }
Init        = { BUILD | QUICK }
StripeSize  = { 8 | 16 | 32 | 64 | 128 | 256 | 512 | 1024 | 2048 | 4096 }

; Array paramters
Array_Mode = { AUTO | CUSTOM }

Array_Defaults  = variance:hotspares

Array.A = { {chanbus:id}+ | {driveNum}+ } | ALL
Array.B = { {chanbus:id}+ | {driveNum}+ } | ALL
Array.C = { {chanbus:id}+ | {driveNum}+ } | ALL
…

Hotspares = { {chanbus:id}+ | {driveNum}+ }

; Logical-drive parameters
Logical_Mode = { AUTO | CUSTOM }

Logical_Defaults = size:raidlevel(:writecmode)

Logical.1 = array:size:raidlevel(:writecmode)
Logical.2 = array:size:raidlevel(:writecmode)
Logical.3 = array:size:raidlevel(:writecmode)
…
	
[Policy.name]
…
	
